{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["QUOTATION"],"not_rendered":{"charts":0,"images":5,"macros":0,"external_links":1,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"QUOTATION","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[[46,2,47,3],[46,7,47,7],[38,1,38,5],[38,6,38,7],[40,2,40,3],[41,2,41,3],[42,2,42,3],[43,2,43,3],[36,2,36,5],[25,2,25,3],[26,2,26,3],[27,2,27,3],[28,2,28,3],[29,2,29,3],[30,2,30,3],[31,2,31,3],[32,2,32,3],[33,2,33,3],[34,2,34,3],[35,2,35,3],[24,2,24,3],[1,1,1,7],[4,2,4,3],[4,4,4,6],[5,2,5,3],[5,4,5,6],[7,2,8,4],[7,7,8,7],[9,2,9,4],[9,6,9,7],[21,2,21,3],[22,2,22,3],[23,2,23,3]]}
[null,"QUOTATION REQUEST - AL AMEEN FOR HUMANITARIAN SUPPORT "]
[null,"طلب عرض سعر"]
[]
[]
[null,null,"PR date:",null,"18-3-2024",null,null,"تاريخ طلب الشراء:"]
[null,null,"\nReference of the PR:\n",null,"PR/ID95H23/World Vision2.28/GZT/PRO-HE/18-3-2024/Zar+Jan-3",null,null,"الرقم المرجعي لطلب الشراء:"]
[]
[null,null,"Quotation valid* from ....../......./........... until ....../......./...........",null,null,null,null,"صلاحية عرض السعر* من ....../......./........... إلى ....../......./..........."]
[]
[null,null,"*Please note that quotation cannot be valid for less than 3 days or more than 30 days. ",null,null,null," ملاحظة : عرض السعر يكون غير صالح لمدة أقل من ثلاثة أيام أو أكثر من 30 يوم."]
[null,null,"Company:",null,null,null,null,"الشركة/المؤسسة:"]
[]
[null,null,"Representative:",null,null,null,null,"اسم الشخص المسؤول:"]
[]
[null,null,"Tel:",null,null,null,null,"الهاتف:"]
[]
[null,null,"Email:",null,null,null,null,"البريد الالكتروني:"]
[]
[null,null,"Address:",null,null,null,null,"العنوان:"]
[]
[]
[null,null,"Items\nالعناصر",null,"Unit\nالواحدة","Quantity\nالكمية","Unit Price in USD includes taxes and delivery\nالسعر الإفرادي","Total Price in USD includes taxes and delivery السعر الإجمالي متضمناً الضريبة والتوصيل"]
[null,1,"Hematology analyzer   Compact size, 22 parameters, 3 Histograms, HD touch screen,  72 samples per hour, 2 reagent system (Diluent & Lyse).",null,"PCs",1]
[null,2,"Microscope   Binocular Microscope, Mechanical Stage, 4 x Objective Lenses, 2 x 10x Wide-Field Eyepieces",null,"PCs",1]
[null,3,"Tow probe connectors portable Ultrasound   15\" high resolution LCD monitor, 2 probe, scanning modes: B, Colour, PW, Power, M, FreeXros M, image display modes: B, 2B, 4B, B/C, B/M, B/PW, Triplex PW, applications: ABD/OB/GYN/CAR/SML/URO/VAS/ORTH/EM/NERVE, transducer variety: Convex, Linear, Micro-convex, endocavity, extended scanning angle with ExFov function, high-frequency linear probe for superficial scanning.",null,"PCs",2]
[null,4,"Infant Warmer( Radiator)   microcontroller-based radiant warmer with manual and servo options should have the facility to display skin set, skin observed temperature\nin degree C and heat power separately, audiovisual alarm facility for overheating beyond set temperature range, alarm facility for patient temperature less than or greater than the required temperature i-e above or below the set range.",null,"PCs",1]
[null,5,"Dry Heat Sterilizer   suitable to operate in temperature range of 160°C-180°C to 250°C/270°C, chamber is constructed for stainless steel 316 is having taper to achieve proper air circulation in sterilizer.\nAll inside contact parts are of stainless steel.",null,"PCs",1]
[null,6,"Patient Monitor with base   Modular & Suitable for Adult/Paediatric/ Patients monitoring , Minimum 15 inches multi color TET display screen, Eight Channel digital and waveforms/ traces display, Facility to monitor and display – ECG, Respiration, NIBP, SpO2, EtCO2, Temp",null,"PCs",1]
[null,7,"ECG Machine   7 \"display, standard 12 leads, Automatic: 3CH×4+1R, 3CH×4, 3CHx2+2CHx3,3CHx2+2CHx3+1R,6CHX2;\nManual: 3CH, 2CH, 3CH+1R, 2CH+1R;\nRhythm: Any lead selectable. \t\nThermal printing system",null,"PCs",1]
[null,8,"Suction Machine   Power supply: 230-240V/50HzVacuum capacity: 18 litres/mim\nMaximum depression: -75kPa (-563mmHg)",null,"PCs",1]
[null,9,"Dressing Table   Stainess Steel Construction\n2 Drawer\n1 x 75mm dia. Swivel castor",null,"PCs",2]
[null,10,"Laryngoscope   Stainless steel handle\nMiller blades: Sizes 1\nMacintosh Blades: Sizes 2, 3 and 4\nWhite PVC case\n2 x C Cell Alkaline Batteries",null,"PCs",1]
[null,11,"Portable light source   Heavy base with low centre of gravity.\nSingle light head with LED lights in cluster.\nArticulating arm between light and base stand.\nPower requirements: 100 - 240 Volts - 50/60 Hz.",null,"PCs",1]
[null,12,"Dental Curing Light   Built-in LED broadband light curing machine, 1 second/3 second fast curing, 4 working modes, high light intensity/progressive light/pulse, metal light guide rod, drop resistant/crack resistan",null,"PCs",1]
[null,13,"Rotary   \nPower: 20 W. Spray output: 3. Noise level: < 70 dBa. Head diameter: 12.5 mm.\nHead size: 13.1 mm. Rotational speed: 380,000 - 450,000 rpm.\nLight: LED. Light intensity: 21 klux approx. Weight: 70 gr.\nConnection: Multiflex. Guarantee: 2 years.",null,"PCs",1]
[null,14,"Otoscope   \nHandle with a built-in LED light source in a mounted head.\nIncluding rotatable viewing lens with a magnification between 3 times.\nColour temperature: Cool white in the range 3,200-4,000K.\nIncluding reusable, autoclavable specula.\nSpecula are cleanable with alcohol wipes\nHandle contains on/off switch.\nIncludes a port to connect an insufflation bulb.\nUses 2 x type AA Alkaline batteries as a power source.\nIs able to withstand frequent cleaning and disinfecting with hospital grade products.",null,"PCs",2]
[null,null,"Total ( المجموع)"]
[]
[null," Comments/Technical specifications:",null,null,null,null,":التعليقات/المواصفات التقنية "]
[]
[null,null,"Total price (in letter)\n",null,null,null,null," السعر الكلي ( في هذا العرض) :"]
[null,null,"Available now:\n",null,null,null,null," كل العناصر متوفرة:"]
[null,null,"The requested quantity is entirely available\n",null,null,null,null," الكمية المطلوبة متوفرة :"]
[null,null,"Delivery date\n",null,null,null,null," تاريخ التسليم:"]
[]
[]
[null,null,"\nSupplier's signature and stamp: \n \n \n",null,null,null,null,"\n ختم وتوقيع المورد : "]